; 
; ITEATAPI.INF
; 
; INF file of IT8211 ATA/ATAPI controller for Windows
; Copyright (c) 2004-2010 Integrated Technology Express, Inc. All rights reserved
;

[Version]
Signature="$Windows NT$"
Provider=%ITE%
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
CatalogFile=iteatapi.cat
DriverVer=05/22/2007,1.3.3.0

[DestinationDirs]
DefaultDestDir = 12             ; DIRID_DRIVERS (this is IOSubsys on
                                ; Win95, and System32\Drivers on NT)

;
; Driver information
;

[Manufacturer]
%ITE%   = ITE.Mfg

[ITE.Mfg]
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_82111283	; 8211/DX
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_2A1D103C	; ASUS OEM
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_81381043	; ASUS 8211
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_2C0717F2	; Albatron 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_B0011458	; Gigabyte 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_B0011940	; Gigabyte 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0A46174B	; 8211/DX
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_90261695	; Epox 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_2801270F	; chaintech 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C25105B	; Foxconn 8212-project 925A02
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C2F105B	; Foxconn 8212-project 915A3.0-2.0.
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_82121019	; ECS
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0CC0105B	; Foxconn LDM01 
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0CC1105B	; Foxconn GWA01 
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C2D105B	; Foxconn project 915A04
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_100E1919     ; Soltek SL-915GPRO-FGR
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_100F1919     ; Soltek SL-915GPRO-DDR2
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_10171919     ; Soltek SL-925PRO-FDGR
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_10181919     ; Soltek SL-915PRO-FGR
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_72001565     ; BIOSTAR 8211
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7A105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7B105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7C105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7D105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7E105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7F105B     ; foxconn 8212
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_1035147B	; ABIT GD8
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_1055147B	; ABIT GD8-M
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_82111849	; ASROCK 8211/DX
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_72001565     ; BIOSTAR 8211
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_1036147B	; ABIT GD8-V
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_1056147B	; ABIT GD8-MV
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0573A0A0	; Aopen 945
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8A105B	; foxconn TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8B105B	; foxconn TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8C105B	; foxconn TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8D105B	; foxconn TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8E105B	; foxconn 945A02
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8F105B	; foxconn TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C0F105B	; Foxconn 875A02
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C25105B	; Foxconn 925A02
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C2D105B	; Foxconn 915A04
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C2F105B	; Foxconn 915A03
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7F105B	; Foxconn 945A01
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7F105B	; Foxconn 945A01
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7A105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7B105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7C105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7D105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C7E105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8A105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8B105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8C105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8D105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8F105B	;  TBD
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0C8E105B	; Foxconn 945A02
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0CC0105B	; Foxconn LPM01
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_0CC1105B	; Foxconn GWA01
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_82118086     ; Intel 8211
%ITE.DeviceDesc0% = iteatapi, PCI\VEN_1283&DEV_8211&SUBSYS_8211107B     ; Intel 8211
;
; General installation section
;

[iteatapi]
AddReg=iteatapi.AddReg
CopyFiles=iteatapi.Miniport
Reboot

[iteatapi.AddReg]

;
; File sections
;

[iteatapi.Miniport]
iteatapi.sys

;
; Service Installation
;

[iteatapi.Services]
AddService = iteatapi, 0x00000002 , iteatapi_Service_Inst, iteatapi_EventLog_Inst

[iteatapi_Service_Inst]
DisplayName    = %iteatapi.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 0                  ; SERVICE_SYSTEM_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
LoadOrderGroup = SCSI Miniport
ServiceBinary  = %12%\iteatapi.sys
AddReg         = pnpsafe_pci_addreg

[iteatapi_EventLog_Inst]
AddReg = iteatapi_EventLog_AddReg

[iteatapi_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\iteatapi.sys"
HKR,,TypesSupported,0x00010001,7

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

;
; Source file information
;

[SourceDisksNames.x86]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iteatapi.sys = 1,,

[Strings]
ITE.DeviceDesc0 = "ITE IT8211 ATA/ATAPI Controller"
DiskId1 = "ITE IT8211 ATA/ATAPI Controller Driver Diskette"
ITE = "ITE Tech, Inc."
iteatapi.SvcDesc="ITEATAPI_Service_Install"